[version.28.5.33] 2012/6/29
1. Add NormalIspParamAddr in xxxx_profile.ini to support normal ISP DRAM parameter 
   download address

[version.28.5.31] 2012/6/25
1. Add DRAM parameter download function for normal ISP

[version.28.5.28]
1. Fix: Card ISP eMMC type pack incorrect
2. Fix: Card ISP pack align size calculation error

[version2.8.5.27]
1. Add interface to query image size

[version2.5.8.21] [DLL:2.8.3.6]: 2011/04/02
1. Unify the method to create Program All image (by external tool)
2. Check if .NET 2.0 exists on FRIM initialization and quit if it doesn't exist

[version2.5.8.20] [DLL:2.8.3.6]: 2010/12/16
1. fixed the bug in 2.8.5.18
2. add DotNetFramework detect for create diskImage

[version2.5.8.18] [DLL:2.8.3.6]: 2010/12/16
1. delete the read verify folder directly, not put it in recycle bin
2. if A, B not used, then alloc size 0 for them.( remove the auto generate A, B 
   function ,and not download PSW file in A )

[version2.8.5.17] [DLL:2.8.3.6]: 2010/11/26
1. fix the timeout bug in nand badblock test & upload. You can specify the 
   timeoutInSeconds item in frm_base.ini( in second uint )

[version2.8.5.16] [DLL:2.8.3.6]: 2010/06/17
1. add rawC pack for "Program All Disk Image"

[version2.8.5.15] [DLL:2.8.3.6]: 2010/06/01
1. add backup filelist for CardUpdate
